**Before the**

**Federal Communications Commission**

**Washington, D.C. 20554**

|  |  |  |
| --- | --- | --- |
| In the Matter ofCreation of Interstitial 12.5 kHz Channels in the 800 MHz Band Between 809-817/854-862 MHz | **)****)****)****)** | WP Docket No. 15-32RM-11572 |

**ERRATUM**

 **Released: March 10, 2015**

By the Deputy Chief, Policy and Licensing Division, Public Safety and Homeland Security Bureau:

On February 9, 2015, the Commission released a *Notice of Proposed Rulemaking (NPRM)*, FCC 15-17, in the above-captioned proceeding.[[1]](#footnote-1) This Erratum amends Appendix B of the *NPRM* as indicated below:

1. On page 47, paragraph 5, which inadvertently referenced 47 C.F.R. § 90.614(a), is removed and the remaining paragraphs are renumbered accordingly.
2. On page 54, below Table C6 of section 90.619, add paragraph (7) and Table C7, which were inadvertently omitted, to read as follows:

(7) \* \* \*

 Table C7—General Category 806-821/851-866 MHz Band Channels in the Canada Border Regions

|  |  |  |
| --- | --- | --- |
| **Canada border region** | **General category channels where 800 MHz high densitycellular systemsare prohibited** | **General category channels where 800 MHz high densitycellular systemsare permitted**  |
| \*\*\*\*\* | \*\*\* | \*\*\* |
| \*\*\*\*\* | \*\*\* | \*\*\* |
| \*\*\*\*\* | \*\*\*-500a | \*\*\* |
| \*\*\*\*\* | \*\*\*-260a, \*\*\* | \*\*\* |
| \*\*\*\*\* | \*\*\* | \*\*\* |

 FEDERAL COMMUNICATIONS COMMISSION

Michael J. Wilhelm

 Deputy Chief

 Policy and Licensing Division

 Public Safety and Homeland Security Bureau

1. The corrected version will be published in the FCC Record. In addition, the corrected version will be posted on the Commission’s website. [↑](#footnote-ref-1)